Product Specifications – Harvesting Chassis Kit (Mobile Chassis + Lifting Platform)
	Design Dimensions
	2330×1925×660 mm
	External Power Supply
	BAT 48V/30A, 24V/30A

	Gross Vehicle Weight
	300 kg (chassis) + 353 kg (lifting platform)
	Braking Method
	Motor braking

	Structure
	Four-wheel drive, four-wheel steering
	Parking Method
	Motor parking + electromagnetic brake (power-off parking)

	Suspension
	No suspension
	Vertical Load (level ground)
	300 kg

	Ground Clearance
	114 mm
	Operating Speed
	7.2 km/h

	Wheelbase
	1750 mm
	Wading Depth
	130 mm

	Track Width
	1570 mm
	Range
	40 km (no load) / 30 km (full load)

	Tire Diameter
	418 mm
	Max. Climbing Angle
	30° (no load) / 10° (full load)

	Drive Motors
	1.2 kW × 4
	Trench Crossing Width
	300 mm (no load) / 200 mm (full load)

	Battery
	48V / 82.5Ah lithium iron phosphate (LiFePO4) battery
	Obstacle Clearance Height
	110 mm (no load) / 50 mm (full load)

	Charging Time
	4–6 h
	Protection Rating
	IP44

	Charging Method
	54.6V/20A manual charging plug
	Communication
	CAN 2.0B

	Lifting Height
	1800 mm
	Platform Deck Dimensions
	1500 mm × 1150 mm






